| BlueSpray - Help © SchoonerTurtles, Inc. 2012-2015
Introduction
Contents
Getting Started
Download
Navigating
Tutorials
Scripting
Advanced
About
| # Class STSRS Extends STContent Defines a reference system for spatially referenced data. A valid SRS will always have a GCS (STGCS). A projected SRS will have a project system (STProjectionSystem). This could be one of: - STPCSValues - a custom projected system - STUTM - STStatePlane - STPCSEPSGCode Copyright, SchoonerTurtles LLP, 2009 @author Jim Graham #### Static Functions
Returns | Function | Throws
--- | --- | ---
STSRS | NewEPSG(int NewEPSGCode) | Exception
STSRS | NewGeographic(STGCS TheGCS) | Exception
STSRS | NewGoogleMercator() | Exception
STSRS | NewStatePlane(STGCS TheGCS,String State,String Zone, STLinearUnit LinearUnit) | Exception
STSRS | NewUTM(STGCS TheGCS,int UTMZone,boolean South) | Exception
## Static Functions ### STSRS NewEPSG(int NewEPSGCode) Exception ### STSRS NewGeographic(STGCS TheGCS) Exception ### STSRS NewGoogleMercator() Exception ### STSRS NewStatePlane(STGCS TheGCS,String State,String Zone, STLinearUnit LinearUnit) Exception ### STSRS NewUTM(STGCS TheGCS,int UTMZone,boolean South) Exception Creates a new STSRS set the the specified UTM zone. Parameters: TheGCS UTMZone South Returns: Throws: Exception