# apnhum46sp

## Shapefile

Description | Spatial | Attributes

Keywords
Theme: Parcels, Ownership, Existing Land Use
Description
Abstract

    Humboldt County's Parcel Layer Version 4.6.  This dataset is the result of an ongoing effort to produce an accurate county wide parcel layer.  Digitizing began as far back as 1996.  Includes all unincorporated areas as well as cities/incorporated areas.  Cities data obtained from Arcata, Eureka, and Trinidad.  Please note the accuracy of GIS map data varies from location to location in the County. This GIS system is useful for planning purposes but should not be relied upon to determine property, zoning or general plan designation boundaries or be used in any way for project design.  All GIS data should be verified before it is materially relied upon for property or project planning.

Purpose

    To be used for planning purposes as general guide to parcel lines within Humboldt County.   Should not be used for boundary delineation or project design.

Supplementary Information

    Updates/History/Corrections:
    This dataset is the result of an ongoing effort to produce a county
    wide parcel layer.  Digitizing began as far back as 1996.
    More recently - 2000 to 2001 - digitizing effort has been increased
    in order to complete this dataset.  Many corrections have been made
    to this dataset, using PLS lines, USGS Quads, Aerial photographs,
    and other sources where available.  Most topological descrepencies
    have been corrected in this dataset.  This data has been reviewed
    for spatial accuracy relative to the PLS lines as well as USGS 7.5
    quads in some areas.  This is the first version of the Humboldt County
    Parcel dataset that will need future review and revisions.  Land use
    attributes - exlu2 & exlu4 - have been added.  Existing Land Use
    values - exlu4 - were created using an interpretive method.
    Zoning, use codes, land ownership, and other information pertaining to
    parcels were used to create "existing" land use categories.

    Jan. 2003 - Cities of Eureka and Rio Dell parcels were added to layer.
    Orleans and Willow Creek have been corrected.
    March 2003 - Cities of Blue Lake and Fortuna were added to layer.
    Hydesville area has been correct using DOQQ's.
    March - April 2003 APN's were checked and corrected for many
    parcels throughout the county.
    Aug. 2003 - Updated Assessor Parcels were incorporated into dataset.
    Jan. 2004 - Updated Assessor Parcels were incorporated into dataset.
    Sept. 2004 - Added 14 missing Parcels for Williamson Contract mapping.
    Dec. 2004 - Re-aligned parcels for the railroad right of way between
    Eureka and Arcata along HWY 101.  Fixed page 20338 parcel numbers.

    May 2005 - Updated Assessor Parcels were incorporated into dataset
    - plotting and plotting2.  City of Trinidad parcel lines were incorporated
    into dataset - trin_par4.  Re-aligned parcels from an outside consultantwere incorporated into dataset - mb.  See [source] attribute.
    Abbreviated Existing Land Use [exlu2] attribute was deleted.
    Existing Land Use [exlu4] attributes were updated for those parcels that changed from vacant to improved or vice versa.

    June 2005 - Eel Delta/Salt River - eeld - and Bridgeville Corrections - brgvl -incorporated into dataset.  Few minor corrections near
    intersection of Ridgewood Dr and Westgate Dr, South Eureka.

    July 2005 - Updated City of Eureka Parcels were incorporated into dataset - [source] = "eka062305".  Significant re-alignment and
    adjustments were made to parcel lines in the areas of McKinleyville,
    Manila, Samoa, Fairhaven, Myrtletown, Cutten, Ridgewood Heights, and
    Elk River using aerial photographs, Assessor Maps, and Section Lines -
    [source] = "cl072705".

    Aug. 12, 2005 - 30704108 fixed.

    Aug. 24, 2005 - Parcels near Arcata/McKinleyville Airport fixed and adjusted.  Parcels west of Rohnerville Airport adjusted.
    [Source] = 'cl082405'

    Sept. 8, 2005 - redigitized in apn #10621205,03. Corrected parcels near Fernbridge.

    December 28, 2005 (clewis) - Updated Assessor Parcels were incorporated into dataset - plotting4 [source] = "ez20050830".  Re-alignment adjustments were made to parcel lines in McKinleyville, South Eureka, Humboldt Hill, Hookton, Briceland, Garberville, & Benbow - [source] = "cl20051221".  New date format adopted for source edits attributes - yyyymmdd.  Apn's 21224201, 02 fixed.

    February 8, 2006 (clewis) - Updated Assessor Parcels were incorporated into
    dataset - plotting5 [source] = "jvd20051212".

    July 12, 2006 (clewis) -  Updated Assessor Parcels were incorporated into dataset - plotting7 [source] = "jvd2006*".  Minor adjustments were made to parcel lines for areas in McKinleyville, Freshwater and Willow Creek using NAIP Imagery.

    Sept. 18, 2006 (clewis) - Updated Assessor Parcels were incorporated into dataset - plotting8.  Adjustments were made to parcel lines for areas of Glendale, Fieldbrook, Manila and Clam Beach using Assessor Pages and NAIP Imagery.

    June 7, 2007 - Updated Assessor Parcels were incorporated into dataset - plotting9, plotting10, and plotting11.

    Aug. 1, 2007 - Updated Assessor Parcels were incorporated into dataset - plotting12.  Included adjustments for Whitethorn area.

    Sept. 25, 2007 - Updated parcels were incorporated to dataset - plotting 13, 14.

    Nov. 9, 2007 - Updated parcels were merged into dataset - plotting15.  Updated City of Arcata parcels were also merged.

    Dec. 10, 2007 - Updated parcels were merged into dataset - plotting16.  Parcels were re-aligned for Myrtle Ave/Indianola, north of Trinidad and Weott.

    Feb. 22, 2008 - Updated parcels were merged into dataset - plotting17.

    March 21, 2008 - Updated parcels were merged into dataset - plotting18.

    April 4, 2008 - Updated City of Arcata parcels were incorporated into dataset.  Updated parcels were merged into dataset - plotting19.

    June 23, 2008 - Updated parcels were merged into dataset - plotting20.  Orick, Benbow areas, Alderpoint were corrected/adjusted/re-aligned.

    August 12, 2008 - Updated parcels were merged into dataset - plotting21.

    September 5, 2008 - Updated parcels were merged into dataset - plotting22.

    November 6, 2008 - Updated parcels were merged into dataset - plotting23. Fieldbrook, and Northern Garbeville were corrected/adjusted/re-aligned.

    February 27, 2009 - Updated parcels were merged into dataset - plotting24.
    Orick, E. Freshwater, Ridgewood Hts. E. Fortuna, and E. Carlotta were corrected/adjusted/re-aligned.

    September 11, 2009 - Updated parcels were merged into dataset - plotting25.
    NW SixRivers National Forest, Willow Creek North, and North McKinleyville were corrected/adjusted/re-aligned. Updated Assesor Roll Added to Joined version.

    January 28, 2010 - Updated parcels were merged into dataset - plotting26.
    Fixes & Corrections West of Redway, Southern Willow Creek, Cutten and, Myrtle  Updated Assesor Roll Added to Joined version.

    June 3, 2010 -  Updated parcels were merged into dataset - plotting27.
    Fixes & Corrections Northeast of Redway, Willow Creek, North of Honeydew, Norhteast Weott, and Northern McKinleyville

    September 24, 2010 - Updated parcels were merged into dataset - plotting28.
    Fixes & Corrections; Northern Honeydew, East of Humboldt Hill, Fickle Hill Road, Southeast Fortuna, Southern Hoopa Reservation
    Updated Assesor Roll Added to Joined version.

    February 3, 2011 - Updated parcels were merged into dataset - plotting29.
    Fixes & Corrections; Portions of Orleans, McKinleyville, Jacoby Creek, Eureka, and the Garberville Airport Region

    September 19, 2011 -  Updated parcels were merged into dataset - plotting30.
    Fixes & Corrections; Western McKinleyville, Fieldbrook, East of Dinsmore, Northern Miranda, Wood Ranch Area, Redway, Southern Garberville, and Benbow .
    Updated Assesor Roll Added to Joined version.

    October 19, 2012 -  Updated parcels were merged into dataset - plotting31.
    Fixes & Corrections; Orleans, Big Lagoon, McKinleyville areas, Azalea Hts, Jacoby Creek, Martin Slough, South of Blue Lake, Titlow Hill, Willow Creek, Southern Ferndale, East of Fortuna, Larabee Valley,  Nothern Rio Dell Annexation, Scotia and, Redway.
    Updated Assesor Roll 9-27-12 Added to Joined version.

    May 10, 2013 - Updated parcels were merged into dataset - plotting32.
    Fixes & Corrections; Yurok Area, Big Lagoon, Patrick's Point, Westhaven, McKinleyville, Glendale, North Arcata, Bayside & Baywood Golf Course, Myrtletown, Eureka, Kneeland, Freshwater, King Salmon, Northern Fortuna, Centerville Beach, Rio Dell, Petrolia, East Myers Flat, Blocksberg, Redway, South Benbow, Shelter Cove, and East Briceland
    Updated Assesor Roll 5-2-13 Added to Joined version.

_________________
Status of the data
Complete
Data update frequency: Quarterly
Time period for which the data is relevant
Date and time: May 10, 2013
Description:

    publication date

Publication Information
Who created the data: Humboldt County Community Development Services
Date and time: May 10, 2013
_________________
Data storage and access information
File name: apnhum46sp
Type of data: vector digital data
Location of the data:
- \\Clark-dc1\snapgis\GIS1\admin\parcels\current\apnhumsp_joined.shp
Data processing environment: Microsoft Windows XP Version 5.1 (Build 2600) Service Pack 3; ESRI ArcCatalog 9.3.1.3000
Accessing the data
Data format: Shapefile
Size of the data: 16.105 MB
Data transfer size: 15.778 MB
Constraints on accessing and using the data
Access constraints: None.
Use constraints:

    To be used for planning purposes as general guide to parcel lines within Humboldt County.   Should not be used for boundary delineation or project design.  Humboldt County Planning and Building Department makes no guarantee of the accuracy or completeness of this data.  It has not been fully reviewed for accuracy and is intended to be used for planning purposes only.  Humboldt County Planning and Building Department assumes no liability or responsibility in the use,  or misuse, of this data.  While every effort has been made to assure the accuracy of this information, it should be understood that it does not have the force and effect of law, rule, or regulation. Should any difference or error occur, the law will take precedence.

Details about this document
Contents last updated: 20130513 at time 15045400
Who completed this document
Jerry von Dohlen
Humboldt County Planning and Building Department
mailing and physical address:

    3015 H St.

Eureka, CA 95501
707-268-3776 (voice)
707-445-7446 (fax)
jvondohlen@co.humboldt.ca.us
Standards used to create this document
Standard name: FGDC Content Standards for Digital Geospatial Metadata
Standard version: FGDC-STD-001-1998
Time convention used in this document: local time
Metadata profiles defining additonal information
- ESRI Metadata Profile: http://www.esri.com/metadata/esriprof80.html
- ESRI Metadata Profile: http://www.esri.com/metadata/esriprof80.html
- ESRI Metadata Profile: http://www.esri.com/metadata/esriprof80.html
- ESRI Metadata Profile: http://www.esri.com/metadata/esriprof80.html
- ESRI Metadata Profile: http://www.esri.com/metadata/esriprof80.html
Horizontal coordinate system
Projected coordinate system name: NAD_1927_StatePlane_California_I_FIPS_0401
Geographic coordinate system name: GCS_North_American_1927
Details
Grid Coordinate System Name: State Plane Coordinate System 1927
SPCS Zone Identifier: 401
Lambert Conformal Conic Projection
Standard Parallel: 40.000000
Standard Parallel: 41.666667
Longitude of Central Meridian: -122.000000
Latitude of Projection Origin: 39.333333
False Easting: 2000000.000000
False Northing: 0.000000
Planar Coordinate Information
Planar Distance Units: survey feet
Coordinate Encoding Method: coordinate pair
Coordinate Representation
Abscissa Resolution: 0.000000
Ordinate Resolution: 0.000000
Geodetic Model
Horizontal Datum Name: North American Datum of 1927
Ellipsoid Name: Clarke 1866
Semi-major Axis: 6378206.400000
Denominator of Flattening Ratio: 294.978698
_________________
Bounding coordinates
Horizontal
In decimal degrees
West: -124.445666
East: -123.383090
North: 41.474443
South: 39.987514
In projected or local coordinates
Left: 1329702.000921
Right: 1612539.750000
Top: 783128.813205
Bottom: 247467.030695
_________________
Lineage
FGDC lineage
Process step 1
Process description: Dataset copied.
Source used: H:\GIS1\admin\parcels\apnhum39sp_joined
Source used: H:\GIS1\admin\parcels\apnhum40sp_joined
Source used: H:\GIS1\admin\parcels\apnhum42sp_joined
Process step 2
Process description: Metadata imported.
Source used: C:\DOCUME~1\JVONDO~1\LOCALS~1\Temp\xml130.tmp
Process step 3
Process description: Dataset copied.
Source used: H:\GIS1\admin\parcels\apnhum38sp_joined
Process date: 20090819 at time 16243200
Process step 4
Process description: Dataset copied.
Source used: H:\GIS1\admin\parcels\apnhum39sp_joinedCopy
Process date: 20090820 at time 10445300
Process step 5
Process description: Dataset copied.
Source used: C:\Gis1\parcels\current\apnhum39sp_joined
Process date: 20090911 at time 15090400
Process step 6
Process description: Dataset copied.
Source used: H:\GIS1\admin\parcels\apnhum39sp_joined
Process date: 20090911 at time 15322900
Process step 7
Process description: Dataset copied.
Process date: 20090911 at time 16071100
Process step 8
Process description: Metadata imported.
Source used: H:\GIS1\admin\parcels\apnhum39utm83.shp.xml
Process date: 20090929 at time 13220100
Process step 9
Process description: Metadata imported.
Source used: H:\GIS1\admin\parcels\apnhum39sp_joined.shp.xml
Process date: 20090929 at time 13225600
Process step 10
Process description: Metadata imported.
Source used: C:\DOCUME~1\JVONDO~1\LOCALS~1\Temp\xml117.tmp
Process date: 20100128 at time 16202400
Process step 11
Process description: Dataset copied.
Source used: C:\Gis1\parcels\current\apnhum40sp_joined
Process date: 20100129 at time 09044500
Process step 12
Process description: Metadata imported.
Source used: H:\GIS1\admin\parcels\current\apnhum40utm83_joined.xml
Process date: 20100222 at time 16195300
Process step 13
Process description: Dataset copied.
Source used: H:\GIS1\admin\parcels\current\apnhumutm83_joined_4web2
Process date: 20100224 at time 11441600
Process step 14
Process description: Metadata imported.
Source used: H:\GIS1\admin\parcels\current\apnhumutm83_joined.shp.xml
Process date: 20100603 at time 15190500
Process step 15
Process description: Dataset copied.
Source used: H:\GIS1\admin\parcels\current\apnhum41sp_joined
Process date: 20100603 at time 15352700
Process step 16
Process description: Dataset copied.
Source used: H:\GIS1\admin\parcels\current\apnhum41sp
Process date: 20100921 at time 14122400
Process step 17
Process description: Dataset copied.
Source used: H:\GIS1\admin\parcels\current\apnhum42sp
Process date: 20100924
Process step 18
Process description: Dataset copied.
Source used: H:\GIS1\admin\parcels\edits\20100629\apnhum42sp_Merge
Process date: 20100921 at time 15304900
Process step 19
Process description: Dataset copied.
Source used: C:\Gis1\parcels\edits\20100629\apnhum42sp
Process date: 20100922 at time 10180500
Process step 20
Process description: Dataset copied.
Source used: H:\GIS1\admin\parcels\current\apnhum42sp
Process date: 20100922 at time 10364300
Process step 21
Process description: Metadata imported.
Source used: C:\DOCUME~1\JVONDO~1\LOCALS~1\Temp\xml98.tmp
Process date: 20110203 at time 17331900
Process step 22
Process description: Metadata imported.
Source used: H:\GIS1\admin\parcels\current\apnhum43sp_joined.xml
Process date: 20110203 at time 17425200
Process step 23
Process description: Metadata imported.
Source used: H:\GIS1\admin\parcels\current\apnhum43sp.xml
Process date: 20110204 at time 12351900
Process step 24
Process description: Dataset copied.
Source used: H:\GIS1\admin\parcels\current\apnhumsp_joined
Process date: 20110916 at time 14110200
Process step 25
Process description: Dataset copied.
Source used: C:\Gis1\parcels\current\apnhumsp_joined
Process date: 20110916 at time 14114100
Process step 26
Process description: Dataset copied.
Source used: C:\Gis1\parcels\current\apnhum44sp
Process date: 20110916 at time 17335700
Process step 27
Process description: Dataset copied.
Source used: H:\GIS1\admin\parcels\current\apnhum44sp
Process date: 20121019 at time 09362400
Process step 28
Process description: Metadata imported.
Source used: C:\DOCUME~1\JVONDO~1\LOCALS~1\Temp\xml56.tmp
Process date: 20121019 at time 15525300
Process step 29
Process description: Dataset copied.
Source used: C:\Gis1\parcels\current\apnhum45sp
Process date: 20121022 at time 14494100
Process step 30
Process description: Dataset copied.
Source used: H:\GIS1\admin\parcels\current\apnhum45sp
Process date: 20130509 at time 11255900
Process step 31
Process description: Dataset copied.
Source used: H:\GIS1\admin\parcels\current\apnhum46sp
Process date: 20130509 at time 13264300
Process step 32
Process description: Metadata imported.
Source used: C:\Gis1\parcels\edits\20130114\apnhum46sp_Merge.shp.xml
Process date: 20130510 at time 14410200
Process step 33
Process description: Dataset copied.
Source used: C:\Gis1\parcels\current\apnhum46sp_joined
Process date: 20130510 at time 17562500
Process step 34
Process description: Metadata imported.
Source used: C:\Gis1\parcels\current\metadata.xml
Process date: 20130510 at time 17590800
Process step 35
Process description: Dataset copied.
Source used: C:\Gis1\parcels\current\apnhum46sp_joined
Process date: 20130510 at time 18083200
Process step 36
Process description: Dataset copied.
Source used: H:\GIS1\admin\parcels\current\apnhum46sp_joined
Process date: 20130510 at time 18153400
Sources
Source 1: Assessor Parcel Maps (AP Maps)
Scale denominator: 1:400, 1:600, 1:1200
ESRI geoprocessing history
1. Process
Date and time: 20130509 at time 135242
Tool location: C:\Program Files\ArcGIS\ArcToolbox\Toolboxes\Data Management Tools.tbx\Merge
Command issued
Merge C:\Gis1\parcels\edits\20130114\apnhum46sp.shp;C:\Gis1\parcels\edits\20130114\plotting32sp.shp C:\Gis1\parcels\edits\20130114\apnhum46sp_Merge.shp "APN 'APN' true true false 9 Text 0 0 ,First,#,C:\Gis1\parcels\edits\20130114\apnhum46sp.shp,APN,-1,-1,C:\Gis1\parcels\edits\20130114\plotting32sp.shp,APN,-1,-1;AREA 'AREA' true true false 19 Double 6 18 ,First,#,C:\Gis1\parcels\edits\20130114\apnhum46sp.shp,AREA,-1,-1,C:\Gis1\parcels\edits\20130114\plotting32sp.shp,AREA,-1,-1;PERIMETER 'PERIMETER' true true false 19 Double 6 18 ,First,#,C:\Gis1\parcels\edits\20130114\apnhum46sp.shp,PERIMETER,-1,-1,C:\Gis1\parcels\edits\20130114\plotting32sp.shp,PERIMETER,-1,-1;EXLU4 'EXLU4' true true false 40 Text 0 0 ,First,#,C:\Gis1\parcels\edits\20130114\apnhum46sp.shp,EXLU4,-1,-1,C:\Gis1\parcels\edits\20130114\plotting32sp.shp,EXLU4,-1,-1;BKPG 'BKPG' true true false 9 Text 0 0 ,First,#,C:\Gis1\parcels\edits\20130114\apnhum46sp.shp,BKPG,-1,-1,C:\Gis1\parcels\edits\20130114\plotting32sp.shp,BKPG,-1,-1;PARCEL 'PARCEL' true true false 5 Text 0 0 ,First,#,C:\Gis1\parcels\edits\20130114\apnhum46sp.shp,PARCEL,-1,-1,C:\Gis1\parcels\edits\20130114\plotting32sp.shp,PARCEL,-1,-1;ACRES 'ACRES' true true false 19 Double 4 18 ,First,#,C:\Gis1\parcels\edits\20130114\apnhum46sp.shp,ACRES,-1,-1,C:\Gis1\parcels\edits\20130114\plotting32sp.shp,ACRES,-1,-1;SOURCE 'SOURCE' true true false 16 Text 0 0 ,First,#,C:\Gis1\parcels\edits\20130114\apnhum46sp.shp,SOURCE,-1,-1,C:\Gis1\parcels\edits\20130114\plotting32sp.shp,SOURCE,-1,-1;EDITORNAME 'EDITORNAME' true true false 50 Text 0 0 ,First,#,C:\Gis1\parcels\edits\20130114\apnhum46sp.shp,EDITORNAME,-1,-1,C:\Gis1\parcels\edits\20130114\plotting32sp.shp,EDITORNAME,-1,-1;LASTUPDATE 'LASTUPDATE' true true false 8 Date 0 0 ,First,#,C:\Gis1\parcels\edits\20130114\apnhum46sp.shp,LASTUPDATE,-1,-1,C:\Gis1\parcels\edits\20130114\plotting32sp.shp,LASTUPDATE,-1,-1"
2. Process
Date and time: 20130510 at time 182216
Tool location: C:\Program Files\ArcGIS\ArcToolbox\Toolboxes\Data Management Tools.tbx\DeleteField
Command issued
DeleteField H:\GIS1\admin\parcels\current\apnhum46sp.shp OID_;APN_1;OLDAPN;ET_AL;TRANDATE;NAME;ADDRESS1;ADDRESS2;ADDRESS3;CITY;STATE;ZIP;O_PHONE;NEIGHCODE;USECODE;TRA;LAND;IMPR;FIXTURE;COURTALPHA;COURTNUMER;RECPAGE;RECPGSUFF;RECDATE;SITHSNBR;SITHSNBRSF;SITSTDIR;SITSTNAME;SITSTTYPE;SITCITY;SITZIP;SBDVNCODE;PORTION;TRACT;GEN_PLAN;ZONING;ZONEDATE;FRONT;REAR;INTSIDE;EXTSIDE;MAX_BLD_HT;MAX_HT_ACC;MAX_LOT_CV;FRONTAGE;ALLEY;DEVPLAN;CZ;CJ;FZ;FR;SUSPENSE;AC_SQFT;LOTSIZE;BLDGS;DWELL_UNIT;WATER;SEWER;SP_AREA;AGPRES;AQ;GEORPT;SS;AOB;AIRPORT;BIO_RES;ARCH;CENTRCT;CENBLK;HZM;SRA;SRAEXMPTD;ACCESS;PUBLICRD;HW;JT;INT;MULTI_SIT;ENTEREDBY;ENTERDATE;X;OWNOCC;OID1;LUCODE;DESCRIPTIO H:\GIS1\admin\parcels\current\apnhum46sp.shp
_________________
Spatial data quality
Horizontal positional accuracy

    +-50 feet, +-400 feet in any direction

_________________
Spatial data description
Vector data information
ESRI description
apnhum46sp
ESRI feature type: Simple
Geometry type: Polygon
Topology: FALSE
Feature count: 72239
Spatial Index: FALSE
Linear referencing: FALSE
SDTS description
Feature class: SDTS feature type, feature count
- apnhum46sp: G-polygon, 72239
Details for apnhum46sp
Type of object: Feature Class
Number of records: 72239
Attributes
FID
Alias: FID
Data type: OID
Width: 4
Precision: 0
Scale: 0
Definition:

    Internal feature number.

Definition Source:

    ESRI

Shape
Alias: Shape
Data type: Geometry
Width: 0
Precision: 0
Scale: 0
Definition:

    Feature geometry.

Definition Source:

    ESRI

APN
Alias: APN
Data type: String
Width: 9
AREA
Alias: AREA
Data type: Number
Width: 19
Number of decimals: 6
PERIMETER
Alias: PERIMETER
Data type: Number
Width: 19
Number of decimals: 6
EXLU4
Alias: EXLU4
Data type: String
Width: 40
BKPG
Alias: BKPG
Data type: String
Width: 9
PARCEL
Alias: PARCEL
Data type: String
Width: 5
ACRES
Alias: ACRES
Data type: Number
Width: 19
Number of decimals: 4
SOURCE
Alias: SOURCE
Data type: String
Width: 16
EDITORNAME
Alias: EDITORNAME
Data type: String
Width: 50
LASTUPDATE
Alias: LASTUPDATE
Data type: Date
Width: 8
_________________
Overview

    Attributes and Definitions:

    [apn] - 8 digit Assessor Parcel Number
    [Area] - Parcel area in square feet as calculated by GIS in CA State
    Plane Zone 1 NAD27 projection
    [Perimeter] - Parcel perimeter length in feet as calculated by GIS
    in CA State Plane Zone 1 NAD27 projection
    [Exlu4] - Existing Land Use (see above)
    [Bkpg] - Parcel Assessor Book and Page Number, first 3 digits are
    book numbers, last 2 digits are page numbers
    [Parcel] - whether polygon is a parcel ("yes") or not ("")
    [Acres] - Parcel Acres as calculated by GIS, [Area]/43560
    [Source] - Data and/or person who did the digitizing that was used to update parcels from vers. 1.19
    [EditorName] - Logged user id that made the last edit to a particular record/shape.
    [LastUpdate] - Logged edit date for the last edit of a parcticular record/